TABLE 28
Model (B4) > Static Structural (B5) > Solution (B6) > Stress Tool > Results

	Object Name
	Safety Factor

	State
	Solved

	Scope

	Scoping Method
	Geometry Selection

	Geometry
	All Bodies

	Definition

	Type
	Safety Factor

	By
	Time

	Display Time
	Last

	Calculate Time History
	Yes

	Identifier
	

	Suppressed
	No

	Integration Point Results

	Display Option
	Averaged

	Results

	Minimum
	0.38079 

	Minimum Occurs On
	CB_Frame_2_J@Surface-Trim1

	Information

	Time
	1. s

	Load Step
	1

	Substep
	1

	Iteration Number
	1


FIGURE 9
Model (B4) > Static Structural (B5) > Solution (B6) > Stress Tool > Safety Factor > seridina
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FIGURE 10
Model (B4) > Static Structural (B5) > Solution (B6) > Stress Tool > Safety Factor > Zad
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FIGURE 11
Model (B4) > Static Structural (B5) > Solution (B6) > Stress Tool > Safety Factor > Pered

[image: image3.png]B: Static Structural
Pered
Type: Safety Factg

i — )
0.38079 Min .
il




FIGURE 12
Model (B4) > Static Structural (B5) > Solution (B6) > Stress Tool > Safety Factor > Overall
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