Solution (B6)

TABLE 23
Model (B4) > Static Structural (B5) > Solution

	Object Name
	Solution (B6)

	State
	Solved

	Adaptive Mesh Refinement

	Max Refinement Loops
	2.

	Refinement Depth
	2.

	Information

	Status
	Done


TABLE 24
Model (B4) > Static Structural (B5) > Solution (B6) > Solution Information

	Object Name
	Solution Information

	State
	Solved

	Solution Information

	Solution Output
	Solver Output

	Newton-Raphson Residuals
	0

	Update Interval
	5. s

	Display Points
	All

	FE Connection Visibility

	Activate Visibility
	Yes

	Display
	All FE Connectors

	Draw Connections Attached To
	All Nodes

	Line Color
	Connection Type

	Visible on Results
	No

	Line Thickness
	Single

	Display Type
	Lines


TABLE 25
Model (B4) > Static Structural (B5) > Solution (B6) > Results

	Object Name
	Structural Error
	Equivalent Stress

	State
	Solved

	Scope

	Scoping Method
	Geometry Selection

	Geometry
	All Bodies

	Shell
	 
	Top/Bottom

	Layer
	 
	Entire Section

	Definition

	Type
	Structural Error
	Equivalent (von-Mises) Stress

	By
	Time

	Display Time
	Last

	Calculate Time History
	Yes

	Identifier
	

	Suppressed
	No

	Results

	Minimum
	5.0372e-008 mJ
	2.886e-002 MPa

	Maximum
	0.12997 mJ
	656.53 MPa

	Minimum Occurs On
	CB_Frame_2_J
	CB_Frame_2_J@Surface-Offset8[3]

	Maximum Occurs On
	CB_Frame_2_J@Surface-Offset8[4]
	CB_Frame_2_J@Surface-Trim1

	Information

	Time
	1. s

	Load Step
	1

	Substep
	1

	Iteration Number
	1

	Integration Point Results

	Display Option
	 
	Averaged


FIGURE 4
Model (B4) > Static Structural (B5) > Solution (B6) > Structural Error > Figure
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TABLE 26
Model (B4) > Static Structural (B5) > Solution (B6) > Equivalent Stress > Convergences

	Object Name
	Convergence

	State
	Solved

	Definition

	Type
	Maximum

	Allowable Change
	5. %

	Results

	Last Change
	3.2064 %

	Converged
	Yes


FIGURE 5
Model (B4) > Static Structural (B5) > Solution (B6) > Equivalent Stress > Convergence

[image: image2.png]657

65

I
(edw) ssans jusieAinba

£

72

Solution Number




Model (B4) > Static Structural (B5) > Solution (B6) > Equivalent Stress > Convergence

	 
	Equivalent Stress (MPa)
	Change (%)
	Nodes
	Elements

	1
	572.08
	
	11027
	10344

	2
	635.81
	10.552
	18562
	16350

	3
	656.53
	3.2064
	41560
	32857


